 ,Model##other##,Total Cooling Capacity##hvac_cooling_load##british_thermal_units_per_hour,Total Heating Capacity##hvac_heating_load##british_thermal_units_per_hour,Voltage##electrical_potential##volts,Frequency##electrical_frequency##hertz,Phase##other##,Single Unit Length##length##inches,Width##length##inches,Height##length##inches,Refrigerant Used##other##,Refrigerant Charge##force##pounds,Operating Weight##force##pounds,Refrigerant Liquid Connection Diameter##pipe_size##inches,Refrigerant Liquid Connection Offset Left##length##inches,Refrigerant Liquid Connection Offset Front##length##inches,Refrigerant Gas Connection Diameter##pipe_size##inches,Refrigerant Gas Connection Offset Left##length##inches,Refrigerant Gas Connection Offset Front##length##inches,Water Connection Diameter##pipe_size##inches,Water Supply Connection Offset Left##length##inches,Water Supply Connection Offset Bottom##length##inches,Water Return Connection Offset Left##length##inches,Water Return Connection Offset Bottom##length##inches,Condensate Drain Connection Diameter##pipe_size##inches,Condensate Drain Connection Offset Bottom##length##inches,Equipment Power Connection Offset Left##length##inches,Equipment Power Connection Offset Front##length##inches,Clearance Offset Top##Length##Inches,Clearance Offset Front##Length##Inches,Clearance Offset Bottom##Length##Inches,Clearance Offset Back##Length##Inches,Family Load Status##other##,Clearance Type##Other##
"18 Ton, 208V/60Hz/3Ph",RWEYQ216PATJ,216000,243000,208,60,3,30.75,21.6875,39.375,R-410A,29.7,990,0.375,10.75,3.0625,0.75,4.1875,2.6875,1.25,3.75,3,3.75,21.875,0.5,0.75,2,1.6875,11.8125,35.4375,0,19.6875,Valid - Type loaded via type catalog,Include Clearance
"18 Ton, 230V/60Hz/3Ph",RWEYQ216PATJ,216000,243000,230,60,3,30.75,21.6875,39.375,R-410A,29.7,990,0.375,10.75,3.0625,0.75,4.1875,2.6875,1.25,3.75,3,3.75,21.875,0.5,0.75,2,1.6875,11.8125,35.4375,0,19.6875,Valid - Type loaded via type catalog,Include Clearance
"21 Ton, 208V/60Hz/3Ph",RWEYQ252PATJ,252000,283500,208,60,3,30.75,21.6875,39.375,R-410A,34.5,990,0.375,10.75,3.0625,0.875,4.1875,2.6875,1.25,3.75,3,3.75,21.875,0.5,0.75,2,1.6875,11.8125,35.4375,0,19.6875,Valid - Type loaded via type catalog,Include Clearance
"21 Ton, 230V/60Hz/3Ph",RWEYQ252PATJ,252000,283500,230,60,3,30.75,21.6875,39.375,R-410A,34.5,990,0.375,10.75,3.0625,0.875,4.1875,2.6875,1.25,3.75,3,3.75,21.875,0.5,0.75,2,1.6875,11.8125,35.4375,0,19.6875,Valid - Type loaded via type catalog,Include Clearance
